Create an unzipped Multi-Sample Player instrument folder. Render clean PCM WAV files at 44.1 kHz, 16-bit stereo. Name every file with InstrumentName_NoteOctave_VVelocity.wav using note names like C3, CS3, D3, DS3. Keep the folder flat with no nested folders. For melodic instruments, render 16 to 32 roots across the useful range and one or two velocity layers. For 16-pad drum kits, render exactly one sound per chromatic note from C3 through DS4. Trim silence, keep peaks below -1 dBFS, avoid clipping, and make each sample start promptly.
